#MicroXplorer Configuration settings - do not modify
ADC1.Channel-1\#ChannelRegularConversion=ADC_CHANNEL_0
ADC1.IPParameters=Rank-1\#ChannelRegularConversion,master,Channel-1\#ChannelRegularConversion,SamplingTime-1\#ChannelRegularConversion,NbrOfConversionFlag
ADC1.NbrOfConversionFlag=1
ADC1.Rank-1\#ChannelRegularConversion=1
ADC1.SamplingTime-1\#ChannelRegularConversion=ADC_SAMPLETIME_3CYCLES
ADC1.master=1
ADC3.Channel-0\#ChannelRegularConversion=ADC_CHANNEL_8
ADC3.IPParameters=Channel-0\#ChannelRegularConversion
CORTEX_M7.IPParameters=PREFETCH_ENABLE
CORTEX_M7.PREFETCH_ENABLE=1
ETH.IPParameters=MediaInterface,MACAddr
ETH.MACAddr=00\:80\:E1\:00\:E0\:00
ETH.MediaInterface=ETH_MEDIA_INTERFACE_RMII
FREERTOS.FootprintOK=true
FREERTOS.INCLUDE_vTaskDelayUntil=1
FREERTOS.IPParameters=Tasks01,configUSE_APPLICATION_TASK_TAG,configUSE_RECURSIVE_MUTEXES,configUSE_COUNTING_SEMAPHORES,configUSE_IDLE_HOOK,configUSE_MALLOC_FAILED_HOOK,configCHECK_FOR_STACK_OVERFLOW,configTOTAL_HEAP_SIZE,FootprintOK,Mutexes01,INCLUDE_vTaskDelayUntil,configENABLE_FPU,Queues01,configRECORD_STACK_HIGH_ADDRESS,configGENERATE_RUN_TIME_STATS
FREERTOS.Mutexes01=MutexLCD,Dynamic,NULL
FREERTOS.Queues01=Queue_F,8,enum End_type,0,Dynamic,NULL,NULL;Queue_N,8,struct Missile,0,Dynamic,NULL,NULL;Queue_J,8,uint8_t,0,Dynamic,NULL,NULL;Queue_E,8,struct Collision,0,Dynamic,NULL,NULL
FREERTOS.Tasks01=GameMaster,2,1024,f_GameMaster,Default,NULL,Dynamic,NULL,NULL;Joueur_1,1,1024,f_Joueur_1,Default,NULL,Dynamic,NULL,NULL;Block_Enemie,-2,1024,f_block_enemie,Default,NULL,Dynamic,NULL,NULL;Projectile,0,1024,f_projectile,Default,NULL,Dynamic,Dynamic,NULL;HUD,-1,1024,f_HUD,Default,NULL,Dynamic,NULL,NULL;chargeur,-1,128,f_chargeur,Default,NULL,Dynamic,NULL,NULL
FREERTOS.configCHECK_FOR_STACK_OVERFLOW=2
FREERTOS.configENABLE_FPU=1
FREERTOS.configGENERATE_RUN_TIME_STATS=0
FREERTOS.configRECORD_STACK_HIGH_ADDRESS=1
FREERTOS.configTOTAL_HEAP_SIZE=32768
FREERTOS.configUSE_APPLICATION_TASK_TAG=1
FREERTOS.configUSE_COUNTING_SEMAPHORES=1
FREERTOS.configUSE_IDLE_HOOK=1
FREERTOS.configUSE_MALLOC_FAILED_HOOK=1
FREERTOS.configUSE_RECURSIVE_MUTEXES=1
File.Version=6
GPIO.groupedBy=Group By Peripherals
KeepUserPlacement=false
LTDC.ActiveH=272
LTDC.ActiveW=480
LTDC.Alpha_L0=255
LTDC.BlendingFactor1_L0=LTDC_BLENDING_FACTOR1_PAxCA
LTDC.BlendingFactor2_L0=LTDC_BLENDING_FACTOR2_PAxCA
LTDC.FBStartAdress_L0=0xC0000000
LTDC.HBP=13
LTDC.HFP=32
LTDC.HSync=41
LTDC.IPParameters=ActiveW,ActiveH,HSync,HBP,HFP,VSync,Layers,WindowX1_L0,WindowY1_L0,Alpha_L0,BlendingFactor1_L0,BlendingFactor2_L0,FBStartAdress_L0,ImageWidth_L0,PixelFormat_L0,ImageHeight_L0
LTDC.ImageHeight_L0=272
LTDC.ImageWidth_L0=480
LTDC.Layers=0
LTDC.PixelFormat_L0=LTDC_PIXEL_FORMAT_RGB565
LTDC.VSync=10
LTDC.WindowX1_L0=480
LTDC.WindowY1_L0=272
LWIP.Version=v2.1.2_Cube
Mcu.Family=STM32F7
Mcu.IP0=ADC1
Mcu.IP1=ADC3
Mcu.IP10=LWIP
Mcu.IP11=NVIC
Mcu.IP12=RCC
Mcu.IP13=RNG
Mcu.IP14=SYS
Mcu.IP15=TIM1
Mcu.IP16=TIM2
Mcu.IP17=TIM3
Mcu.IP18=TIM5
Mcu.IP19=TIM8
Mcu.IP2=CORTEX_M7
Mcu.IP3=CRC
Mcu.IP4=DAC
Mcu.IP5=DMA2D
Mcu.IP6=ETH
Mcu.IP7=FMC
Mcu.IP8=FREERTOS
Mcu.IP9=LTDC
Mcu.IPNb=20
Mcu.Name=STM32F746NGHx
Mcu.Package=TFBGA216
Mcu.Pin0=PE4
Mcu.Pin1=PE3
Mcu.Pin10=PA13
Mcu.Pin100=PA1
Mcu.Pin101=PA0/WKUP
Mcu.Pin102=PA4
Mcu.Pin103=PC4
Mcu.Pin104=PF13
Mcu.Pin105=PG0
Mcu.Pin106=PJ3
Mcu.Pin107=PE8
Mcu.Pin108=PG5
Mcu.Pin109=PG4
Mcu.Pin11=PE5
Mcu.Pin110=PH7
Mcu.Pin111=PH9
Mcu.Pin112=PH11
Mcu.Pin113=PA2
Mcu.Pin114=PA5
Mcu.Pin115=PC5
Mcu.Pin116=PF14
Mcu.Pin117=PJ2
Mcu.Pin118=PF11
Mcu.Pin119=PE9
Mcu.Pin12=PE6
Mcu.Pin120=PE11
Mcu.Pin121=PE14
Mcu.Pin122=PH6
Mcu.Pin123=PH8
Mcu.Pin124=PH10
Mcu.Pin125=PA3
Mcu.Pin126=PA7
Mcu.Pin127=PB1
Mcu.Pin128=PB0
Mcu.Pin129=PJ0
Mcu.Pin13=PG13
Mcu.Pin130=PJ1
Mcu.Pin131=PE7
Mcu.Pin132=PE10
Mcu.Pin133=PE12
Mcu.Pin134=PE15
Mcu.Pin135=PE13
Mcu.Pin136=PB11
Mcu.Pin137=PB14
Mcu.Pin138=PB15
Mcu.Pin139=VP_CRC_VS_CRC
Mcu.Pin14=PB9
Mcu.Pin140=VP_DMA2D_VS_DMA2D
Mcu.Pin141=VP_FREERTOS_VS_CMSIS_V1
Mcu.Pin142=VP_LWIP_VS_Enabled
Mcu.Pin143=VP_RNG_VS_RNG
Mcu.Pin144=VP_SYS_VS_tim6
Mcu.Pin145=VP_TIM1_VS_ClockSourceINT
Mcu.Pin146=VP_TIM2_VS_ClockSourceINT
Mcu.Pin147=VP_TIM3_VS_ClockSourceINT
Mcu.Pin148=VP_TIM3_VS_ClockSourceITR
Mcu.Pin149=VP_TIM5_VS_ClockSourceINT
Mcu.Pin15=PB7
Mcu.Pin150=VP_TIM8_VS_ClockSourceINT
Mcu.Pin16=PG15
Mcu.Pin17=PG11
Mcu.Pin18=PJ13
Mcu.Pin19=PJ12
Mcu.Pin2=PG14
Mcu.Pin20=PD6
Mcu.Pin21=PD0
Mcu.Pin22=PI8
Mcu.Pin23=PK7
Mcu.Pin24=PK6
Mcu.Pin25=PK5
Mcu.Pin26=PG12
Mcu.Pin27=PJ14
Mcu.Pin28=PD5
Mcu.Pin29=PD3
Mcu.Pin3=PE1
Mcu.Pin30=PD1
Mcu.Pin31=PI3
Mcu.Pin32=PI2
Mcu.Pin33=PC13
Mcu.Pin34=PF0
Mcu.Pin35=PI10
Mcu.Pin36=PK4
Mcu.Pin37=PK3
Mcu.Pin38=PJ15
Mcu.Pin39=PD4
Mcu.Pin4=PE0
Mcu.Pin40=PH15
Mcu.Pin41=PI1
Mcu.Pin42=PC14/OSC32_IN
Mcu.Pin43=PF1
Mcu.Pin44=PI12
Mcu.Pin45=PI9
Mcu.Pin46=PH14
Mcu.Pin47=PI0
Mcu.Pin48=PA9
Mcu.Pin49=PC15/OSC32_OUT
Mcu.Pin5=PB8
Mcu.Pin50=PK1
Mcu.Pin51=PK2
Mcu.Pin52=PA8
Mcu.Pin53=PH0/OSC_IN
Mcu.Pin54=PF2
Mcu.Pin55=PI13
Mcu.Pin56=PI15
Mcu.Pin57=PJ11
Mcu.Pin58=PK0
Mcu.Pin59=PC7
Mcu.Pin6=PB5
Mcu.Pin60=PH1/OSC_OUT
Mcu.Pin61=PF3
Mcu.Pin62=PI14
Mcu.Pin63=PH4
Mcu.Pin64=PJ8
Mcu.Pin65=PJ10
Mcu.Pin66=PG8
Mcu.Pin67=PC6
Mcu.Pin68=PF4
Mcu.Pin69=PH5
Mcu.Pin7=PB4
Mcu.Pin70=PH3
Mcu.Pin71=PJ7
Mcu.Pin72=PJ9
Mcu.Pin73=PG7
Mcu.Pin74=PF7
Mcu.Pin75=PF5
Mcu.Pin76=PH2
Mcu.Pin77=PJ6
Mcu.Pin78=PD15
Mcu.Pin79=PB13
Mcu.Pin8=PA15
Mcu.Pin80=PD10
Mcu.Pin81=PF10
Mcu.Pin82=PF9
Mcu.Pin83=PF8
Mcu.Pin84=PC3
Mcu.Pin85=PD14
Mcu.Pin86=PB12
Mcu.Pin87=PD9
Mcu.Pin88=PD8
Mcu.Pin89=PC0
Mcu.Pin9=PA14
Mcu.Pin90=PC1
Mcu.Pin91=PC2
Mcu.Pin92=PF12
Mcu.Pin93=PG1
Mcu.Pin94=PF15
Mcu.Pin95=PJ4
Mcu.Pin96=PG3
Mcu.Pin97=PG2
Mcu.Pin98=PJ5
Mcu.Pin99=PH12
Mcu.PinsNb=151
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32F746NGHx
MxCube.Version=6.2.1
MxDb.Version=DB.6.0.21
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.ETH_IRQn=true\:5\:0\:false\:false\:true\:true\:false\:true
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.LTDC_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.PendSV_IRQn=true\:15\:0\:false\:false\:false\:true\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:false\:false\:false\:false
NVIC.SavedPendsvIrqHandlerGenerated=true
NVIC.SavedSvcallIrqHandlerGenerated=true
NVIC.SavedSystickIrqHandlerGenerated=true
NVIC.SysTick_IRQn=true\:15\:0\:false\:false\:false\:true\:false\:true
NVIC.TIM6_DAC_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:true
NVIC.TimeBase=TIM6_DAC_IRQn
NVIC.TimeBaseIP=TIM6
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
PA0/WKUP.Locked=true
PA0/WKUP.Signal=ADCx_IN0
PA1.Mode=RMII
PA1.Signal=ETH_REF_CLK
PA13.GPIOParameters=GPIO_Label
PA13.GPIO_Label=SWDIO
PA13.Locked=true
PA13.Mode=Serial_Wire
PA13.Signal=SYS_JTMS-SWDIO
PA14.GPIOParameters=GPIO_Label
PA14.GPIO_Label=SWCLK
PA14.Locked=true
PA14.Mode=Serial_Wire
PA14.Signal=SYS_JTCK-SWCLK
PA15.GPIOParameters=GPIO_Label
PA15.GPIO_Label=BP2
PA15.Locked=true
PA15.Signal=GPIO_Input
PA2.Mode=RMII
PA2.Signal=ETH_MDIO
PA3.GPIOParameters=GPIO_Label
PA3.GPIO_Label=ULPI_D0 [USB3320C-EZK_D0]
PA3.Locked=true
PA3.Mode=Host_HS
PA3.Signal=USB_OTG_HS_ULPI_D0
PA4.Locked=true
PA4.Signal=COMP_DAC1_group
PA5.GPIOParameters=GPIO_Label
PA5.GPIO_Label=ULPI_CLK [USB3320C-EZK_CLKOUT]
PA5.Locked=true
PA5.Mode=Host_HS
PA5.Signal=USB_OTG_HS_ULPI_CK
PA7.Mode=RMII
PA7.Signal=ETH_CRS_DV
PA8.GPIOParameters=GPIO_Label
PA8.GPIO_Label=BP1
PA8.Locked=true
PA8.Signal=GPIO_Input
PA9.GPIOParameters=GPIO_Speed,GPIO_PuPd,GPIO_Label,GPIO_Mode
PA9.GPIO_Label=VCP_TX [STM32F103CBT6_PA3]
PA9.GPIO_Mode=GPIO_MODE_AF_PP
PA9.GPIO_PuPd=GPIO_NOPULL
PA9.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PA9.Locked=true
PA9.Signal=USART1_TX
PB0.GPIOParameters=GPIO_Label
PB0.GPIO_Label=ULPI_D1 [USB3320C-EZK_D1]
PB0.Locked=true
PB0.Mode=Host_HS
PB0.Signal=USB_OTG_HS_ULPI_D1
PB1.GPIOParameters=GPIO_Label
PB1.GPIO_Label=ULPI_D2 [USB3320C-EZK_D2]
PB1.Locked=true
PB1.Mode=Host_HS
PB1.Signal=USB_OTG_HS_ULPI_D2
PB11.GPIOParameters=GPIO_Label
PB11.GPIO_Label=ULPI_D4 [USB3320C-EZK_D4]
PB11.Locked=true
PB11.Mode=Host_HS
PB11.Signal=USB_OTG_HS_ULPI_D4
PB12.GPIOParameters=GPIO_Label
PB12.GPIO_Label=ULPI_D5 [USB3320C-EZK_D5]
PB12.Locked=true
PB12.Mode=Host_HS
PB12.Signal=USB_OTG_HS_ULPI_D5
PB13.GPIOParameters=GPIO_Label
PB13.GPIO_Label=ULPI_D6 [USB3320C-EZK_D6]
PB13.Locked=true
PB13.Mode=Host_HS
PB13.Signal=USB_OTG_HS_ULPI_D6
PB14.Locked=true
PB14.Signal=SPI2_MISO
PB15.Locked=true
PB15.Signal=SPI2_MOSI
PB4.Locked=true
PB4.Signal=S_TIM3_CH1
PB5.GPIOParameters=GPIO_Label
PB5.GPIO_Label=ULPI_D7 [USB3320C-EZK_D7]
PB5.Locked=true
PB5.Mode=Host_HS
PB5.Signal=USB_OTG_HS_ULPI_D7
PB7.GPIOParameters=GPIO_Speed,GPIO_PuPd,GPIO_Label,GPIO_Mode
PB7.GPIO_Label=VCP_RX [STM32F103CBT6_PA2]
PB7.GPIO_Mode=GPIO_MODE_AF_PP
PB7.GPIO_PuPd=GPIO_NOPULL
PB7.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PB7.Locked=true
PB7.Signal=USART1_RX
PB8.GPIOParameters=GPIO_Speed,GPIO_PuPd,GPIO_Label,GPIO_Mode
PB8.GPIO_Label=ARDUINO SCL/D15
PB8.GPIO_Mode=GPIO_MODE_AF_OD
PB8.GPIO_PuPd=GPIO_NOPULL
PB8.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PB8.Locked=true
PB8.Signal=I2C1_SCL
PB9.GPIOParameters=GPIO_Speed,GPIO_PuPd,GPIO_Label,GPIO_Mode
PB9.GPIO_Label=ARDUINO SDA/D14
PB9.GPIO_Mode=GPIO_MODE_AF_OD
PB9.GPIO_PuPd=GPIO_NOPULL
PB9.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PB9.Locked=true
PB9.Signal=I2C1_SDA
PC0.GPIOParameters=GPIO_Label
PC0.GPIO_Label=ULPI_STP [USB3320C-EZK_STP]
PC0.Locked=true
PC0.Mode=Host_HS
PC0.Signal=USB_OTG_HS_ULPI_STP
PC1.Mode=RMII
PC1.Signal=ETH_MDC
PC13.GPIOParameters=GPIO_Label
PC13.GPIO_Label=uSD_Detect
PC13.Locked=true
PC13.Signal=GPIO_Input
PC14/OSC32_IN.GPIOParameters=GPIO_Label
PC14/OSC32_IN.GPIO_Label=RCC_OSC32_IN
PC14/OSC32_IN.Locked=true
PC14/OSC32_IN.Mode=LSE-External-Oscillator
PC14/OSC32_IN.Signal=RCC_OSC32_IN
PC15/OSC32_OUT.GPIOParameters=GPIO_Label
PC15/OSC32_OUT.GPIO_Label=RCC_OSC32_OUT
PC15/OSC32_OUT.Locked=true
PC15/OSC32_OUT.Mode=LSE-External-Oscillator
PC15/OSC32_OUT.Signal=RCC_OSC32_OUT
PC2.GPIOParameters=GPIO_Label
PC2.GPIO_Label=ULPI_DIR [USB3320C-EZK_DIR]
PC2.Locked=true
PC2.Mode=Host_HS
PC2.Signal=USB_OTG_HS_ULPI_DIR
PC3.Mode=SdramChipSelect1_1
PC3.Signal=FMC_SDCKE0
PC4.Mode=RMII
PC4.Signal=ETH_RXD0
PC5.Mode=RMII
PC5.Signal=ETH_RXD1
PC6.Locked=true
PC6.Signal=USART6_TX
PC7.Locked=true
PC7.Signal=USART6_RX
PD0.Signal=FMC_D2_DA2
PD1.Signal=FMC_D3_DA3
PD10.Signal=FMC_D15_DA15
PD14.Signal=FMC_D0_DA0
PD15.Signal=FMC_D1_DA1
PD3.GPIOParameters=GPIO_Label
PD3.GPIO_Label=LED16
PD3.Locked=true
PD3.Signal=GPIO_Output
PD4.GPIOParameters=GPIO_Label
PD4.GPIO_Label=OTG_FS_OverCurrent [STMPS2141STR_Fault]
PD4.Locked=true
PD4.Signal=GPIO_Input
PD5.GPIOParameters=PinState,GPIO_Label
PD5.GPIO_Label=OTG_FS_PowerSwitchOn [STMPS2141STR_EN]
PD5.Locked=true
PD5.PinState=GPIO_PIN_SET
PD5.Signal=GPIO_Output
PD6.GPIOParameters=GPIO_Label,GPIO_ModeDefaultEXTI
PD6.GPIO_Label=Audio_INT
PD6.GPIO_ModeDefaultEXTI=GPIO_MODE_EVT_RISING
PD6.Locked=true
PD6.Signal=GPXTI6
PD8.Signal=FMC_D13_DA13
PD9.Signal=FMC_D14_DA14
PE0.Signal=FMC_NBL0
PE1.Signal=FMC_NBL1
PE10.Signal=FMC_D7_DA7
PE11.Signal=FMC_D8_DA8
PE12.Signal=FMC_D9_DA9
PE13.Signal=FMC_D10_DA10
PE14.Signal=FMC_D11_DA11
PE15.Signal=FMC_D12_DA12
PE3.Locked=true
PE3.Signal=GPIO_Input
PE4.GPIOParameters=GPIO_Label
PE4.GPIO_Label=LCD_B0 [RK043FN48H-CT672B_B0]
PE4.Locked=true
PE4.Mode=RGB888
PE4.Signal=LTDC_B0
PE5.GPIOParameters=GPIO_Label
PE5.GPIO_Label=LED14
PE5.Locked=true
PE5.Signal=GPIO_Output
PE6.GPIOParameters=GPIO_Label
PE6.GPIO_Label=LED15
PE6.Locked=true
PE6.Signal=GPIO_Output
PE7.Signal=FMC_D4_DA4
PE8.Signal=FMC_D5_DA5
PE9.Signal=FMC_D6_DA6
PF0.Signal=FMC_A0
PF1.Signal=FMC_A1
PF10.Locked=true
PF10.Mode=IN8
PF10.Signal=ADC3_IN8
PF11.Signal=FMC_SDNRAS
PF12.Signal=FMC_A6
PF13.Signal=FMC_A7
PF14.Signal=FMC_A8
PF15.Signal=FMC_A9
PF2.Signal=FMC_A2
PF3.Signal=FMC_A3
PF4.Signal=FMC_A4
PF5.Signal=FMC_A5
PF7.Locked=true
PF7.Signal=UART7_TX
PF8.Locked=true
PF8.Signal=ADC3_IN6
PF9.Locked=true
PF9.Signal=ADC3_IN7
PG0.Signal=FMC_A10
PG1.Signal=FMC_A11
PG11.Mode=RMII
PG11.Signal=ETH_TX_EN
PG12.GPIOParameters=GPIO_Label
PG12.GPIO_Label=LCD_B4 [RK043FN48H-CT672B_B4]
PG12.Locked=true
PG12.Mode=RGB888
PG12.Signal=LTDC_B4
PG13.Mode=RMII
PG13.Signal=ETH_TXD0
PG14.Mode=RMII
PG14.Signal=ETH_TXD1
PG15.Signal=FMC_SDNCAS
PG2.GPIOParameters=GPIO_Label
PG2.GPIO_Label=RMII_RXER
PG2.Locked=true
PG2.Signal=GPIO_Input
PG3.GPIOParameters=GPIO_Label
PG3.GPIO_Label=EXT_RST
PG3.Locked=true
PG3.Signal=GPIO_Output
PG4.Signal=FMC_A14_BA0
PG5.Signal=FMC_A15_BA1
PG7.GPIOParameters=GPIO_Label
PG7.GPIO_Label=BP_JOYSTICK
PG7.Locked=true
PG7.Signal=GPIO_Input
PG8.Signal=FMC_SDCLK
PH0/OSC_IN.GPIOParameters=GPIO_Label
PH0/OSC_IN.GPIO_Label=OSC_25M [NZ2520SB-25.00M_OUT]
PH0/OSC_IN.Locked=true
PH0/OSC_IN.Mode=HSE-External-Oscillator
PH0/OSC_IN.Signal=RCC_OSC_IN
PH1/OSC_OUT.Locked=true
PH1/OSC_OUT.Mode=HSE-External-Oscillator
PH1/OSC_OUT.Signal=RCC_OSC_OUT
PH10.GPIOParameters=GPIO_Label
PH10.GPIO_Label=LED18
PH10.Locked=true
PH10.Signal=GPIO_Output
PH11.GPIOParameters=GPIO_Label
PH11.GPIO_Label=LED12
PH11.Locked=true
PH11.Signal=GPIO_Output
PH12.GPIOParameters=GPIO_Label
PH12.GPIO_Label=LED17
PH12.Locked=true
PH12.Signal=GPIO_Output
PH14.GPIOParameters=GPIO_Label
PH14.GPIO_Label=LED13
PH14.Locked=true
PH14.Signal=GPIO_Output
PH15.GPIOParameters=GPIO_Label
PH15.GPIO_Label=TP3
PH15.Locked=true
PH15.Signal=GPIO_Input
PH2.GPIOParameters=GPIO_Label
PH2.GPIO_Label=NC2
PH2.Locked=true
PH2.Signal=GPIO_Input
PH3.Mode=SdramChipSelect1_1
PH3.Signal=FMC_SDNE0
PH4.GPIOParameters=GPIO_Label
PH4.GPIO_Label=ULPI_NXT [USB3320C-EZK_NXT]
PH4.Locked=true
PH4.Mode=Host_HS
PH4.Signal=USB_OTG_HS_ULPI_NXT
PH5.Signal=FMC_SDNWE
PH6.GPIOParameters=GPIO_Label
PH6.GPIO_Label=LED2
PH6.Locked=true
PH6.Signal=GPIO_Output
PH7.GPIOParameters=GPIO_Label
PH7.GPIO_Label=LCD_SCL [RK043FN48H-CT672B_SCL]
PH7.Locked=true
PH7.Signal=I2C3_SCL
PH8.GPIOParameters=GPIO_Label
PH8.GPIO_Label=LCD_SDA [RK043FN48H-CT672B_SDA]
PH8.Locked=true
PH8.Signal=I2C3_SDA
PH9.GPIOParameters=GPIO_Label
PH9.GPIO_Label=LED11
PH9.Locked=true
PH9.Signal=GPIO_Output
PI0.Locked=true
PI0.Signal=SPI2_NSS
PI1.GPIOParameters=GPIO_Speed,GPIO_PuPd,GPIO_Label,GPIO_Mode
PI1.GPIO_Label=ARDUINO SCK/D13
PI1.GPIO_Mode=GPIO_MODE_AF_PP
PI1.GPIO_PuPd=GPIO_NOPULL
PI1.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PI1.Locked=true
PI1.Signal=SPI2_SCK
PI10.GPIOParameters=GPIO_Label
PI10.GPIO_Label=LCD_HSYNC [RK043FN48H-CT672B_HSYNC]
PI10.Locked=true
PI10.Mode=RGB888
PI10.Signal=LTDC_HSYNC
PI12.GPIOParameters=PinState,GPIO_Label
PI12.GPIO_Label=LCD_DISP [RK043FN48H-CT672B_DISP] 
PI12.Locked=true
PI12.PinState=GPIO_PIN_SET
PI12.Signal=GPIO_Output
PI13.GPIOParameters=GPIO_Label,GPIO_ModeDefaultEXTI
PI13.GPIO_Label=LCD_INT
PI13.GPIO_ModeDefaultEXTI=GPIO_MODE_EVT_RISING
PI13.Locked=true
PI13.Signal=GPXTI13
PI14.GPIOParameters=GPIO_Label
PI14.GPIO_Label=LCD_CLK [RK043FN48H-CT672B_CLK]
PI14.Locked=true
PI14.Mode=RGB888
PI14.Signal=LTDC_CLK
PI15.GPIOParameters=GPIO_Label
PI15.GPIO_Label=LCD_R0 [RK043FN48H-CT672B_R0]
PI15.Locked=true
PI15.Mode=RGB888
PI15.Signal=LTDC_R0
PI2.Locked=true
PI2.Signal=S_TIM8_CH4
PI3.GPIOParameters=GPIO_Label
PI3.GPIO_Label=LED3
PI3.Locked=true
PI3.Signal=GPIO_Output
PI8.GPIOParameters=GPIO_Label
PI8.GPIO_Label=NC1 [TP2]
PI8.Locked=true
PI8.Signal=RTC_TS
PI9.GPIOParameters=GPIO_Label
PI9.GPIO_Label=LCD_VSYNC [RK043FN48H-CT672B_VSYNC]
PI9.Locked=true
PI9.Mode=RGB888
PI9.Signal=LTDC_VSYNC
PJ0.GPIOParameters=GPIO_Label
PJ0.GPIO_Label=LCD_R1 [RK043FN48H-CT672B_R1]
PJ0.Locked=true
PJ0.Mode=RGB888
PJ0.Signal=LTDC_R1
PJ1.GPIOParameters=GPIO_Label
PJ1.GPIO_Label=LCD_R2 [RK043FN48H-CT672B_R2]
PJ1.Locked=true
PJ1.Mode=RGB888
PJ1.Signal=LTDC_R2
PJ10.GPIOParameters=GPIO_Label
PJ10.GPIO_Label=LCD_G3 [RK043FN48H-CT672B_G3]
PJ10.Locked=true
PJ10.Mode=RGB888
PJ10.Signal=LTDC_G3
PJ11.GPIOParameters=GPIO_Label
PJ11.GPIO_Label=LCD_G4 [RK043FN48H-CT672B_G4]
PJ11.Locked=true
PJ11.Mode=RGB888
PJ11.Signal=LTDC_G4
PJ12.GPIOParameters=GPIO_Label
PJ12.GPIO_Label=OTG_FS_VBUS
PJ12.Locked=true
PJ12.Signal=GPIO_Input
PJ13.GPIOParameters=GPIO_Label
PJ13.GPIO_Label=LCD_B1 [RK043FN48H-CT672B_B1]
PJ13.Locked=true
PJ13.Mode=RGB888
PJ13.Signal=LTDC_B1
PJ14.GPIOParameters=GPIO_Label
PJ14.GPIO_Label=LCD_B2 [RK043FN48H-CT672B_B2]
PJ14.Locked=true
PJ14.Mode=RGB888
PJ14.Signal=LTDC_B2
PJ15.GPIOParameters=GPIO_Label
PJ15.GPIO_Label=LCD_B3 [RK043FN48H-CT672B_B3]
PJ15.Locked=true
PJ15.Mode=RGB888
PJ15.Signal=LTDC_B3
PJ2.GPIOParameters=GPIO_Label
PJ2.GPIO_Label=LCD_R3 [RK043FN48H-CT672B_R3]
PJ2.Locked=true
PJ2.Mode=RGB888
PJ2.Signal=LTDC_R3
PJ3.GPIOParameters=GPIO_Label
PJ3.GPIO_Label=LCD_R4 [RK043FN48H-CT672B_R4]
PJ3.Locked=true
PJ3.Mode=RGB888
PJ3.Signal=LTDC_R4
PJ4.GPIOParameters=GPIO_Label
PJ4.GPIO_Label=LCD_R5 [RK043FN48H-CT672B_R5]
PJ4.Locked=true
PJ4.Mode=RGB888
PJ4.Signal=LTDC_R5
PJ5.GPIOParameters=GPIO_Label
PJ5.GPIO_Label=LCD_R6 [RK043FN48H-CT672B_R6]
PJ5.Locked=true
PJ5.Mode=RGB888
PJ5.Signal=LTDC_R6
PJ6.GPIOParameters=GPIO_Label
PJ6.GPIO_Label=LCD_R7 [RK043FN48H-CT672B_R7]
PJ6.Locked=true
PJ6.Mode=RGB888
PJ6.Signal=LTDC_R7
PJ7.GPIOParameters=GPIO_Label
PJ7.GPIO_Label=LCD_G0 [RK043FN48H-CT672B_G0]
PJ7.Locked=true
PJ7.Mode=RGB888
PJ7.Signal=LTDC_G0
PJ8.GPIOParameters=GPIO_Label
PJ8.GPIO_Label=LCD_G1 [RK043FN48H-CT672B_G1]
PJ8.Locked=true
PJ8.Mode=RGB888
PJ8.Signal=LTDC_G1
PJ9.GPIOParameters=GPIO_Label
PJ9.GPIO_Label=LCD_G2 [RK043FN48H-CT672B_G2]
PJ9.Locked=true
PJ9.Mode=RGB888
PJ9.Signal=LTDC_G2
PK0.GPIOParameters=GPIO_Label
PK0.GPIO_Label=LCD_G5 [RK043FN48H-CT672B_G5]
PK0.Locked=true
PK0.Mode=RGB888
PK0.Signal=LTDC_G5
PK1.GPIOParameters=GPIO_Label
PK1.GPIO_Label=LCD_G6 [RK043FN48H-CT672B_G6]
PK1.Locked=true
PK1.Mode=RGB888
PK1.Signal=LTDC_G6
PK2.GPIOParameters=GPIO_Label
PK2.GPIO_Label=LCD_G7 [RK043FN48H-CT672B_G7]
PK2.Locked=true
PK2.Mode=RGB888
PK2.Signal=LTDC_G7
PK3.GPIOParameters=GPIO_Speed,PinState,GPIO_Label
PK3.GPIO_Label=LCD_BL_CTRL [STLD40DPUR_EN]
PK3.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PK3.Locked=true
PK3.PinState=GPIO_PIN_SET
PK3.Signal=GPIO_Output
PK4.GPIOParameters=GPIO_Label
PK4.GPIO_Label=LCD_B5 [RK043FN48H-CT672B_B5]
PK4.Locked=true
PK4.Mode=RGB888
PK4.Signal=LTDC_B5
PK5.GPIOParameters=GPIO_Label
PK5.GPIO_Label=LCD_B6 [RK043FN48H-CT672B_B6]
PK5.Locked=true
PK5.Mode=RGB888
PK5.Signal=LTDC_B6
PK6.GPIOParameters=GPIO_Label
PK6.GPIO_Label=LCD_B7 [RK043FN48H-CT672B_B7]
PK6.Locked=true
PK6.Mode=RGB888
PK6.Signal=LTDC_B7
PK7.GPIOParameters=GPIO_Label
PK7.GPIO_Label=LCD_DE [RK043FN48H-CT672B_DE]
PK7.Locked=true
PK7.Mode=RGB888
PK7.Signal=LTDC_DE
PinOutPanel.CurrentBGAView=Top
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=true
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32F746NGHx
ProjectManager.FirmwarePackage=STM32Cube FW_F7 V1.16.1
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=Space_Invaders.ioc
ProjectManager.ProjectName=Space_Invaders
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-MX_GPIO_Init-GPIO-false-HAL-true,2-SystemClock_Config-RCC-false-HAL-false,3-MX_ADC3_Init-ADC3-false-HAL-true,4-MX_LTDC_Init-LTDC-false-HAL-true,5-MX_TIM1_Init-TIM1-false-HAL-true,6-MX_TIM2_Init-TIM2-false-HAL-true,7-MX_TIM3_Init-TIM3-false-HAL-true,8-MX_TIM5_Init-TIM5-false-HAL-true,9-MX_TIM8_Init-TIM8-false-HAL-true,10-MX_DAC_Init-DAC-false-HAL-true,11-MX_FMC_Init-FMC-false-HAL-true,12-MX_DMA2D_Init-DMA2D-false-HAL-true,13-MX_CRC_Init-CRC-false-HAL-true,14-MX_RNG_Init-RNG-false-HAL-true,15-MX_LWIP_Init-LWIP-false-HAL-false,16-MX_ADC1_Init-ADC1-false-HAL-true,0-MX_CORTEX_M7_Init-CORTEX_M7-false-HAL-true
RCC.AHBFreq_Value=200000000
RCC.APB1CLKDivider=RCC_HCLK_DIV4
RCC.APB1Freq_Value=50000000
RCC.APB1TimFreq_Value=100000000
RCC.APB2CLKDivider=RCC_HCLK_DIV2
RCC.APB2Freq_Value=100000000
RCC.APB2TimFreq_Value=200000000
RCC.CECFreq_Value=32786.88524590164
RCC.CortexFreq_Value=200000000
RCC.EthernetFreq_Value=200000000
RCC.FCLKCortexFreq_Value=200000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=200000000
RCC.HSE_VALUE=25000000
RCC.HSI_VALUE=16000000
RCC.I2C1Freq_Value=50000000
RCC.I2C2Freq_Value=50000000
RCC.I2C3Freq_Value=50000000
RCC.I2C4Freq_Value=50000000
RCC.I2SFreq_Value=50000000
RCC.IPParameters=AHBFreq_Value,APB1CLKDivider,APB1Freq_Value,APB1TimFreq_Value,APB2CLKDivider,APB2Freq_Value,APB2TimFreq_Value,CECFreq_Value,CortexFreq_Value,EthernetFreq_Value,FCLKCortexFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI_VALUE,I2C1Freq_Value,I2C2Freq_Value,I2C3Freq_Value,I2C4Freq_Value,I2SFreq_Value,LCDTFToutputFreq_Value,LPTIM1Freq_Value,LSI_VALUE,MCO2PinFreq_Value,PLL48CLockSelection,PLLCLKFreq_Value,PLLI2SN,PLLI2SPCLKFreq_Value,PLLI2SQCLKFreq_Value,PLLI2SRCLKFreq_Value,PLLI2SRoutputFreq_Value,PLLM,PLLN,PLLQ,PLLQCLKFreq_Value,PLLQoutputFreq_Value,PLLSAIN,PLLSAIP,PLLSAIPCLKFreq_Value,PLLSAIQCLKFreq_Value,PLLSAIR,PLLSAIRCLKFreq_Value,PLLSAIRDiv,PLLSAIoutputFreq_Value,PLLSourceVirtual,RNGFreq_Value,SAI1Freq_Value,SAI2Freq_Value,SDMMCClockSelection,SDMMCFreq_Value,SPDIFRXFreq_Value,SYSCLKFreq_VALUE,SYSCLKSource,UART4Freq_Value,UART5Freq_Value,UART7Freq_Value,UART8Freq_Value,USART1Freq_Value,USART2Freq_Value,USART3Freq_Value,USART6Freq_Value,USBFreq_Value,VCOI2SOutputFreq_Value,VCOInputFreq_Value,VCOOutputFreq_Value,VCOSAIOutputFreq_Value
RCC.LCDTFToutputFreq_Value=9600000
RCC.LPTIM1Freq_Value=50000000
RCC.LSI_VALUE=32000
RCC.MCO2PinFreq_Value=200000000
RCC.PLL48CLockSelection=RCC_CLK48SOURCE_PLLSAIP
RCC.PLLCLKFreq_Value=200000000
RCC.PLLI2SN=100
RCC.PLLI2SPCLKFreq_Value=50000000
RCC.PLLI2SQCLKFreq_Value=50000000
RCC.PLLI2SRCLKFreq_Value=50000000
RCC.PLLI2SRoutputFreq_Value=50000000
RCC.PLLM=25
RCC.PLLN=400
RCC.PLLQ=9
RCC.PLLQCLKFreq_Value=44444444.44444445
RCC.PLLQoutputFreq_Value=44444444.44444445
RCC.PLLSAIN=384
RCC.PLLSAIP=RCC_PLLSAIP_DIV8
RCC.PLLSAIPCLKFreq_Value=48000000
RCC.PLLSAIQCLKFreq_Value=192000000
RCC.PLLSAIR=5
RCC.PLLSAIRCLKFreq_Value=76800000
RCC.PLLSAIRDiv=RCC_PLLSAIDIVR_8
RCC.PLLSAIoutputFreq_Value=48000000
RCC.PLLSourceVirtual=RCC_PLLSOURCE_HSE
RCC.RNGFreq_Value=48000000
RCC.SAI1Freq_Value=192000000
RCC.SAI2Freq_Value=192000000
RCC.SDMMCClockSelection=RCC_SDMMC1CLKSOURCE_CLK48
RCC.SDMMCFreq_Value=48000000
RCC.SPDIFRXFreq_Value=50000000
RCC.SYSCLKFreq_VALUE=200000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.UART4Freq_Value=50000000
RCC.UART5Freq_Value=50000000
RCC.UART7Freq_Value=50000000
RCC.UART8Freq_Value=50000000
RCC.USART1Freq_Value=100000000
RCC.USART2Freq_Value=50000000
RCC.USART3Freq_Value=50000000
RCC.USART6Freq_Value=100000000
RCC.USBFreq_Value=48000000
RCC.VCOI2SOutputFreq_Value=100000000
RCC.VCOInputFreq_Value=1000000
RCC.VCOOutputFreq_Value=400000000
RCC.VCOSAIOutputFreq_Value=384000000
SH.ADCx_IN0.0=ADC1_IN0,IN0
SH.ADCx_IN0.ConfNb=1
SH.COMP_DAC1_group.0=DAC_OUT1,DAC_OUT1
SH.COMP_DAC1_group.ConfNb=1
SH.FMC_A0.0=FMC_A0,12b-sda1
SH.FMC_A0.ConfNb=1
SH.FMC_A1.0=FMC_A1,12b-sda1
SH.FMC_A1.ConfNb=1
SH.FMC_A10.0=FMC_A10,12b-sda1
SH.FMC_A10.ConfNb=1
SH.FMC_A11.0=FMC_A11,12b-sda1
SH.FMC_A11.ConfNb=1
SH.FMC_A14_BA0.0=FMC_BA0,FourSdramBanks1
SH.FMC_A14_BA0.ConfNb=1
SH.FMC_A15_BA1.0=FMC_BA1,FourSdramBanks1
SH.FMC_A15_BA1.ConfNb=1
SH.FMC_A2.0=FMC_A2,12b-sda1
SH.FMC_A2.ConfNb=1
SH.FMC_A3.0=FMC_A3,12b-sda1
SH.FMC_A3.ConfNb=1
SH.FMC_A4.0=FMC_A4,12b-sda1
SH.FMC_A4.ConfNb=1
SH.FMC_A5.0=FMC_A5,12b-sda1
SH.FMC_A5.ConfNb=1
SH.FMC_A6.0=FMC_A6,12b-sda1
SH.FMC_A6.ConfNb=1
SH.FMC_A7.0=FMC_A7,12b-sda1
SH.FMC_A7.ConfNb=1
SH.FMC_A8.0=FMC_A8,12b-sda1
SH.FMC_A8.ConfNb=1
SH.FMC_A9.0=FMC_A9,12b-sda1
SH.FMC_A9.ConfNb=1
SH.FMC_D0_DA0.0=FMC_D0,sd-16b-d1
SH.FMC_D0_DA0.ConfNb=1
SH.FMC_D10_DA10.0=FMC_D10,sd-16b-d1
SH.FMC_D10_DA10.ConfNb=1
SH.FMC_D11_DA11.0=FMC_D11,sd-16b-d1
SH.FMC_D11_DA11.ConfNb=1
SH.FMC_D12_DA12.0=FMC_D12,sd-16b-d1
SH.FMC_D12_DA12.ConfNb=1
SH.FMC_D13_DA13.0=FMC_D13,sd-16b-d1
SH.FMC_D13_DA13.ConfNb=1
SH.FMC_D14_DA14.0=FMC_D14,sd-16b-d1
SH.FMC_D14_DA14.ConfNb=1
SH.FMC_D15_DA15.0=FMC_D15,sd-16b-d1
SH.FMC_D15_DA15.ConfNb=1
SH.FMC_D1_DA1.0=FMC_D1,sd-16b-d1
SH.FMC_D1_DA1.ConfNb=1
SH.FMC_D2_DA2.0=FMC_D2,sd-16b-d1
SH.FMC_D2_DA2.ConfNb=1
SH.FMC_D3_DA3.0=FMC_D3,sd-16b-d1
SH.FMC_D3_DA3.ConfNb=1
SH.FMC_D4_DA4.0=FMC_D4,sd-16b-d1
SH.FMC_D4_DA4.ConfNb=1
SH.FMC_D5_DA5.0=FMC_D5,sd-16b-d1
SH.FMC_D5_DA5.ConfNb=1
SH.FMC_D6_DA6.0=FMC_D6,sd-16b-d1
SH.FMC_D6_DA6.ConfNb=1
SH.FMC_D7_DA7.0=FMC_D7,sd-16b-d1
SH.FMC_D7_DA7.ConfNb=1
SH.FMC_D8_DA8.0=FMC_D8,sd-16b-d1
SH.FMC_D8_DA8.ConfNb=1
SH.FMC_D9_DA9.0=FMC_D9,sd-16b-d1
SH.FMC_D9_DA9.ConfNb=1
SH.FMC_NBL0.0=FMC_NBL0,Sd2ByteEnable1
SH.FMC_NBL0.ConfNb=1
SH.FMC_NBL1.0=FMC_NBL1,Sd2ByteEnable1
SH.FMC_NBL1.ConfNb=1
SH.FMC_SDCLK.0=FMC_SDCLK,12b-sda1
SH.FMC_SDCLK.ConfNb=1
SH.FMC_SDNCAS.0=FMC_SDNCAS,12b-sda1
SH.FMC_SDNCAS.ConfNb=1
SH.FMC_SDNRAS.0=FMC_SDNRAS,12b-sda1
SH.FMC_SDNRAS.ConfNb=1
SH.FMC_SDNWE.0=FMC_SDNWE,12b-sda1
SH.FMC_SDNWE.ConfNb=1
SH.GPXTI13.0=GPIO_EXTI13
SH.GPXTI13.ConfNb=1
SH.GPXTI6.0=GPIO_EXTI6
SH.GPXTI6.ConfNb=1
SH.S_TIM3_CH1.0=TIM3_CH1,PWM Generation1 CH1
SH.S_TIM3_CH1.ConfNb=1
SH.S_TIM8_CH4.0=TIM8_CH4,PWM Generation4 CH4
SH.S_TIM8_CH4.ConfNb=1
TIM3.Channel-PWM\ Generation1\ CH1=TIM_CHANNEL_1
TIM3.IPParameters=Channel-PWM Generation1 CH1
TIM8.Channel-PWM\ Generation4\ CH4=TIM_CHANNEL_4
TIM8.IPParameters=Channel-PWM Generation4 CH4
VP_CRC_VS_CRC.Mode=CRC_Activate
VP_CRC_VS_CRC.Signal=CRC_VS_CRC
VP_DMA2D_VS_DMA2D.Mode=DMA2D_Activate
VP_DMA2D_VS_DMA2D.Signal=DMA2D_VS_DMA2D
VP_FREERTOS_VS_CMSIS_V1.Mode=CMSIS_V1
VP_FREERTOS_VS_CMSIS_V1.Signal=FREERTOS_VS_CMSIS_V1
VP_LWIP_VS_Enabled.Mode=Enabled
VP_LWIP_VS_Enabled.Signal=LWIP_VS_Enabled
VP_RNG_VS_RNG.Mode=RNG_Activate
VP_RNG_VS_RNG.Signal=RNG_VS_RNG
VP_SYS_VS_tim6.Mode=TIM6
VP_SYS_VS_tim6.Signal=SYS_VS_tim6
VP_TIM1_VS_ClockSourceINT.Mode=Internal
VP_TIM1_VS_ClockSourceINT.Signal=TIM1_VS_ClockSourceINT
VP_TIM2_VS_ClockSourceINT.Mode=Internal
VP_TIM2_VS_ClockSourceINT.Signal=TIM2_VS_ClockSourceINT
VP_TIM3_VS_ClockSourceINT.Mode=Internal
VP_TIM3_VS_ClockSourceINT.Signal=TIM3_VS_ClockSourceINT
VP_TIM3_VS_ClockSourceITR.Mode=TriggerSource_ITR0
VP_TIM3_VS_ClockSourceITR.Signal=TIM3_VS_ClockSourceITR
VP_TIM5_VS_ClockSourceINT.Mode=Internal
VP_TIM5_VS_ClockSourceINT.Signal=TIM5_VS_ClockSourceINT
VP_TIM8_VS_ClockSourceINT.Mode=Internal
VP_TIM8_VS_ClockSourceINT.Signal=TIM8_VS_ClockSourceINT
board=STM32F746G-DISCO
boardIOC=true
isbadioc=false
